EB185 ARM Board driver.
Matrix Multimedia Ltd. may 2006

Hardware: Matrix ARM Board Drivers EB031/EB034/EB185 (EB185 = EB031 and EB034 in combination).
For: Windows 2000, XP and Vista.


To install for Windows 2000, XP, 2003 and Vista:
Run Driver installation before plugging in hardware.
Run ARMBoardDriverInstaller.exe and follow the instructions provided.



For Windows 98/ME

Plug in the hardware board and set to program mode (see product datasheet).
The New hardware wizard will then launch.
Select the 'Specify a location' option and point the install wizard to this folder.
Select mx_eb031.inf file.
Follow the instructions to install the drivers. 