Stationery.zip and freemaster_demo.zip.
 
The Stationery.zip contains 4 following 56F8006 stationeries:
56F8006_32_LQFP_JTAG
56F8006_32_LQFP_SCI
56F8006_48_LQFP_JTAG
56F8006_48_LQFP_SCI
 
If you build a new project on that stationery above it will contain integrated and enabled Freemaster Serial Driver.(it is not required to add the driver manually then as described in the presentation).
The FreeMASTER stationeries support 32 LQFP and 48 LQFP packages.
For each package both SCI and JTAG configurations are provided.
The JTAG version works only in POLLING MODE. It is not provided to configure AW OnCE interrupts using Processor Expert (PE). 
Using the FreeMASTER JTAG interface in polling mode if the JTAG interface is desired instead of the serial.

The SCI versions run at 38400 Bd. 
Due to MC56F8006 errata 2, the  CMXUSB RS232 emullator on JM60 is unstable at 115200Bd. Therefore use 38400.  In general, higher baud rates are not required for Freemaster.
 
The freemaster_demo.zip file contains very basic example of FreeMASTER usage.
It demonstrates  WATCH, SCOPE and RECORDER features. To watch the example double click demo.pmp file. It will start the FreeMASTER windows client.



