FreeMASTER Serial Communication Driver 56F8xxx Digital Signal Controllers
=========================================================================

This folder contains the 56F8xxx platform-dependent part of 
FreeMASTER serial communication driver. Please see the User Manual for 
more information about how to configure and use the driver.


Driver example/test applications available in <install_path>/examples folder:
(<install_path> is typically C:\Program Files\FreeMASTER Serial Communication)

<install_path>/examples/56F8xxx/56F8346EVM_qs
---------------------------------------------
- Freescale 56F8346EVM development board
- CodeWarrior 56800/E Hybrid Controllers version 7.2
- The application is based on DSP56F800E_Quick_Start r2.0, all Quick_Start
  source code is copied into the application so it is not required to 
  have Quick_Start installed (although Graphical Configuration Tool 
	of QS may help to re-configure the application if needed).
  
<install_path>/examples/56F8xxx/DEMO56F8013_qs
----------------------------------------------
- Freescale DEMO56F8013 development board
- CodeWarrior 56800/E Hybrid Controllers version 7.2
- The application is based on DSP56F800E_Quick_Start r2.0, all Quick_Start
  source code is copied into the application so it is not required to 
  have Quick_Start installed (although Graphical Configuration Tool 
	of QS may help to re-configure the application if needed).

  
----
Copyright (c) 1999-2006, Freescale Semiconductor Inc.
Freescale Transportation & Standard Products Group
ALL RIGHTS RESERVED, www.freescale.com
